- Main Page
- Data Structures
- Files
- Directories

- Data Structures
- Data Fields

# XIsf_FlashToBufTransferParam Struct Reference

`#include <xilisf.h>`

## Data Fields
u8 | BufferNum
u32 | Address

## Detailed Description

The following structure definition specifies the operational parameters to be passed to the XIsf_Read API while performing Page to Buffer Transfer operation (XISF_PAGE_TO_BUF_TRANS) in Atmel Serial Flash.

## Field Documentation

u32 XIsf_FlashToBufTransferParam::Address

| Start address in the Serial Flash

u8 XIsf_FlashToBufTransferParam::BufferNum

| SRAM buffer number of Serial Flash

The documentation for this struct was generated from the following file:

- xilisf.h