- Main Page
- Data Structures
- Files
- Directories

- Data Structures
- Data Fields

# XIsf_BufferToFlashWriteParam Struct Reference

`#include <xilisf.h>`

## Data Fields
u8 | BufferNum
u32 | Address

## Detailed Description

The following structure definition specifies the operational parameters to be passed to the XIsf_Write API while writing data from the internal SRAM buffer to a Page in the Atmel Serial Flash using XISF_BUF_TO_PAGE_WRITE_WITH_ERASE / XISF_BUF_TO_PAGE_WRITE_WITHOUT_ERASE commands in Atmel Serial Flash.

## Field Documentation

u32 XIsf_BufferToFlashWriteParam::Address

| Starting address in the Serial Flash

u8 XIsf_BufferToFlashWriteParam::BufferNum

| SRAM buffer number of Serial Flash

The documentation for this struct was generated from the following file:

- xilisf.h