- Main Page
- Data Structures
- Files
- Directories

- Data Structures
- Data Fields

# XIsf_ReadParam Struct Reference

`#include <xilisf.h>`

## Data Fields
u32 | Address
u8 * | ReadPtr
u32 | NumBytes
int | NumDummyBytes

## Detailed Description

The following structure definition specifies the operational parameters to be passed to the XIsf_Read API while performing Normal Read (XISF_READ), Fast Read (XISF_FAST_READ) and OTP Read (XISF_OTP_READ) operations .

## Field Documentation

u32 XIsf_ReadParam::Address

| Start address in the Serial Flash

u32 XIsf_ReadParam::NumBytes

| Number of bytes to read

int XIsf_ReadParam::NumDummyBytes

| Number of dummy bytes associated with the fast read command. Valid only for dual o/p fast read, dual i/o fast read, quad o/p fast read and quad i/o fast read

u8* XIsf_ReadParam::ReadPtr

| Read buffer pointer where data needs to be stored

The documentation for this struct was generated from the following file:

- xilisf.h