<?xml version="1.0" encoding="UTF-8" standalone="no" ?>
<bd:repository xmlns:bd="http://www.xilinx.com/bd" bd:isValidated="true" bd:synthFlowMode="None" bd:tool_version="2015.1" bd:top="tutorial" bd:version="1.00.a">

  <spirit:component xmlns:spirit="http://www.spiritconsortium.org/XMLSchema/SPIRIT/1685-2009">
    <spirit:vendor>xilinx.com</spirit:vendor>
    <spirit:library>BlockDiagram</spirit:library>
    <spirit:name>tutorial</spirit:name>
    <spirit:version>1.00.a</spirit:version>
    <spirit:parameters>
      <spirit:parameter>
        <spirit:name>isTop</spirit:name>
        <spirit:value spirit:format="bool" spirit:resolve="immediate">true</spirit:value>
      </spirit:parameter>
    </spirit:parameters>
    <spirit:busInterfaces>
      <spirit:busInterface>
        <spirit:name>DDR</spirit:name>
        <spirit:master/>
        <spirit:busType spirit:library="interface" spirit:name="ddrx" spirit:vendor="xilinx.com" spirit:version="1.0"/>
        <spirit:abstractionType spirit:library="interface" spirit:name="ddrx_rtl" spirit:vendor="xilinx.com" spirit:version="1.0"/>
      </spirit:busInterface>
      <spirit:busInterface>
        <spirit:name>FIXED_IO</spirit:name>
        <spirit:master/>
        <spirit:busType spirit:library="display_processing_system7" spirit:name="fixedio" spirit:vendor="xilinx.com" spirit:version="1.0"/>
        <spirit:abstractionType spirit:library="display_processing_system7" spirit:name="fixedio_rtl" spirit:vendor="xilinx.com" spirit:version="1.0"/>
      </spirit:busInterface>
      <spirit:busInterface>
        <spirit:name>ARD_I2C1</spirit:name>
        <spirit:master/>
        <spirit:busType spirit:library="interface" spirit:name="iic" spirit:vendor="xilinx.com" spirit:version="1.0"/>
        <spirit:abstractionType spirit:library="interface" spirit:name="iic_rtl" spirit:vendor="xilinx.com" spirit:version="1.0"/>
      </spirit:busInterface>
    </spirit:busInterfaces>
    <spirit:model>
      <spirit:views>
        <spirit:view>
          <spirit:name>BlockDiagram</spirit:name>
          <spirit:envIdentifier>:vivado.xilinx.com:</spirit:envIdentifier>
          <spirit:hierarchyRef spirit:library="BlockDiagram" spirit:name="tutorial_imp" spirit:vendor="xilinx.com" spirit:version="1.00.a"/>
        </spirit:view>
      </spirit:views>
      <spirit:ports>
        <spirit:port>
          <spirit:name>SDIO1_CDN</spirit:name>
          <spirit:wire>
            <spirit:direction>in</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>UART0_RTSN</spirit:name>
          <spirit:wire>
            <spirit:direction>out</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>UART0_TX</spirit:name>
          <spirit:wire>
            <spirit:direction>out</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>UART0_CTSN</spirit:name>
          <spirit:wire>
            <spirit:direction>in</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>UART0_RX</spirit:name>
          <spirit:wire>
            <spirit:direction>in</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>BT_EN_SOC</spirit:name>
          <spirit:wire>
            <spirit:direction>out</spirit:direction>
            <spirit:vector>
              <spirit:left>0</spirit:left>
              <spirit:right>0</spirit:right>
            </spirit:vector>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>ARD_RELAY</spirit:name>
          <spirit:wire>
            <spirit:direction>out</spirit:direction>
            <spirit:vector>
              <spirit:left>3</spirit:left>
              <spirit:right>0</spirit:right>
            </spirit:vector>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>ARD_SPI1_MOSI</spirit:name>
          <spirit:wire>
            <spirit:direction>out</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>ARD_SPI1_MISO</spirit:name>
          <spirit:wire>
            <spirit:direction>in</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>ARD_SPI1_SCLK</spirit:name>
          <spirit:wire>
            <spirit:direction>out</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>ARD_SPI1_SS</spirit:name>
          <spirit:wire>
            <spirit:direction>out</spirit:direction>
          </spirit:wire>
        </spirit:port>
        <spirit:port>
          <spirit:name>ARD_SPI1_DC</spirit:name>
          <spirit:wire>
            <spirit:direction>out</spirit:direction>
            <spirit:vector>
              <spirit:left>0</spirit:left>
              <spirit:right>0</spirit:right>
            </spirit:vector>
          </spirit:wire>
        </spirit:port>
      </spirit:ports>
    </spirit:model>
  </spirit:component>

  <spirit:design xmlns:spirit="http://www.spiritconsortium.org/XMLSchema/SPIRIT/1685-2009">
    <spirit:vendor>xilinx.com</spirit:vendor>
    <spirit:library>BlockDiagram</spirit:library>
    <spirit:name>tutorial_imp</spirit:name>
    <spirit:version>1.00.a</spirit:version>
    <spirit:componentInstances>
      <spirit:componentInstance>
        <spirit:instanceName>processing_system7_0</spirit:instanceName>
        <spirit:componentRef spirit:library="ip" spirit:name="processing_system7" spirit:vendor="xilinx.com" spirit:version="5.5"/>
        <spirit:configurableElementValues>
          <spirit:configurableElementValue spirit:referenceId="bd:xciName">tutorial_processing_system7_0_0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_DDR_RAM_HIGHADDR">0x3FFFFFFF</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_0">-0.073</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_1">-0.072</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_2">0.024</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_3">0.023</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_BOARD_DELAY0">0.294</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_BOARD_DELAY1">0.298</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_BOARD_DELAY2">0.338</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_BOARD_DELAY3">0.334</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQS_0_LENGTH_MM">50.05</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQS_1_LENGTH_MM">50.43</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQS_2_LENGTH_MM">50.10</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQS_3_LENGTH_MM">50.01</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQ_0_LENGTH_MM">49.59</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQ_1_LENGTH_MM">51.74</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQ_2_LENGTH_MM">50.32</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_DQ_3_LENGTH_MM">48.55</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_CLOCK_0_LENGTH_MM">39.7</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_CLOCK_1_LENGTH_MM">39.7</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_CLOCK_2_LENGTH_MM">54.14</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_CLOCK_3_LENGTH_MM">54.14</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_0">-0.112</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_1">-0.093</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_2">0.019</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_3">0.009</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PACKAGE_DDR_BOARD_DELAY0">0.361</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PACKAGE_DDR_BOARD_DELAY1">0.351</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PACKAGE_DDR_BOARD_DELAY2">0.386</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PACKAGE_DDR_BOARD_DELAY3">0.391</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SDIO_PERIPHERAL_FREQMHZ">50</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UART_PERIPHERAL_FREQMHZ">50</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_FPGA0_PERIPHERAL_FREQMHZ">75.000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_FPGA1_PERIPHERAL_FREQMHZ">150.000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_FPGA2_PERIPHERAL_FREQMHZ">100.000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ACT_QSPI_PERIPHERAL_FREQMHZ">200.000000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ACT_ENET0_PERIPHERAL_FREQMHZ">125.000000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ACT_SDIO_PERIPHERAL_FREQMHZ">50.000000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ACT_UART_PERIPHERAL_FREQMHZ">50.000000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ACT_FPGA0_PERIPHERAL_FREQMHZ">76.923080</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ACT_FPGA1_PERIPHERAL_FREQMHZ">142.857132</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ACT_FPGA2_PERIPHERAL_FREQMHZ">100.000000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_CLK0_FREQ">76923080</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_CLK1_FREQ">142857132</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_CLK2_FREQ">100000000</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SDIO_PERIPHERAL_VALID">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_EMIO_TTC0">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_USE_M_AXI_GP0">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_USE_S_AXI_HP0">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_USE_DMA0">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_USE_FABRIC_INTERRUPT">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_QSPI">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_ENET0">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_GPIO">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_SDIO0">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_UART1">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_TTC0">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_USB0">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_CLK0_PORT">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_CLK1_PORT">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_CLK2_PORT">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_CLK3_PORT">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_EN_RST1_PORT">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PERIPHERAL_BOARD_PRESET">part0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PRESET_BANK1_VOLTAGE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_PARTNO">MT41K256M16 RE-125</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_TRAIN_WRITE_LEVEL">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_TRAIN_READ_GATE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_TRAIN_DATA_EYE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UIPARAM_DDR_USE_INTERNAL_VREF">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_QSPI_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_QSPI_QSPI_IO">MIO 1 .. 6</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_QSPI_GRP_SINGLE_SS_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_QSPI_GRP_SINGLE_SS_IO">MIO 1 .. 6</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_QSPI_GRP_FBCLK_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_QSPI_GRP_FBCLK_IO">MIO 8</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ENET0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ENET0_ENET0_IO">MIO 16 .. 27</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ENET0_GRP_MDIO_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_ENET0_GRP_MDIO_IO">MIO 52 .. 53</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD0_SD0_IO">MIO 40 .. 45</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD0_GRP_CD_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD0_GRP_CD_IO">MIO 46</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD0_GRP_WP_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD0_GRP_WP_IO">MIO 50</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD1_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD1_SD1_IO">MIO 10 .. 15</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD1_GRP_CD_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SD1_GRP_CD_IO">EMIO</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UART0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UART0_GRP_FULL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UART1_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_UART1_UART1_IO">MIO 48 .. 49</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_SPI1_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_TTC0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_TTC0_TTC0_IO">EMIO</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_USB0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_USB0_USB0_IO">MIO 28 .. 39</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_USB0_RESET_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_USB0_RESET_IO">MIO 7</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_I2C1_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_GPIO_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_GPIO_MIO_GPIO_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_GPIO_MIO_GPIO_IO">MIO</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_GPIO_EMIO_GPIO_ENABLE">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_GPIO_EMIO_GPIO_IO">6</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_DCI_PERIPHERAL_CLKSRC">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_PCAP_PERIPHERAL_CLKSRC">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_0_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_0_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_0_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_1_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_1_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_1_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_2_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_2_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_3_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_3_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_4_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_4_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_5_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_5_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_6_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_6_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_7_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_7_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_8_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_8_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_9_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_9_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_9_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_10_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_10_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_10_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_11_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_11_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_11_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_12_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_12_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_12_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_13_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_13_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_13_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_14_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_14_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_14_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_15_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_15_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_15_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_16_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_16_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_16_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_17_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_17_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_17_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_18_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_18_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_18_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_19_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_19_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_19_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_20_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_20_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_20_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_21_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_21_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_21_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_22_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_22_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_22_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_23_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_23_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_23_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_24_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_24_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_24_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_25_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_25_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_25_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_26_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_26_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_26_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_27_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_27_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_27_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_28_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_28_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_28_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_29_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_29_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_29_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_30_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_30_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_30_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_31_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_31_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_31_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_32_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_32_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_32_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_33_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_33_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_33_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_34_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_34_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_34_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_35_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_35_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_35_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_36_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_36_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_36_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_37_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_37_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_37_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_38_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_38_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_38_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_39_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_39_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_39_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_40_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_40_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_40_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_41_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_41_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_41_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_42_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_42_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_42_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_43_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_43_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_43_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_44_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_44_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_44_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_45_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_45_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_45_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_46_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_46_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_46_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_47_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_47_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_47_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_48_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_48_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_48_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_49_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_49_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_49_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_50_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_50_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_50_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_51_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_51_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_51_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_52_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_52_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_52_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_53_PULLUP">disabled</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_53_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_53_SLEW">slow</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="preset">Microzed</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_TREE_PERIPHERALS">GPIO#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#USB Reset#Quad SPI Flash#GPIO#SD 1#SD 1#SD 1#SD 1#SD 1#SD 1#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#SD 0#SD 0#SD 0#SD 0#SD 0#SD 0#SD 0#GPIO#UART 1#UART 1#SD 0#GPIO#Enet 0#Enet 0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="PCW_MIO_TREE_SIGNALS">gpio[0]#qspi0_ss_b#qspi0_io[0]#qspi0_io[1]#qspi0_io[2]#qspi0_io[3]#qspi0_sclk#reset#qspi_fbclk#gpio[9]#data[0]#cmd#clk#data[1]#data[2]#data[3]#tx_clk#txd[0]#txd[1]#txd[2]#txd[3]#tx_ctl#rx_clk#rxd[0]#rxd[1]#rxd[2]#rxd[3]#rx_ctl#data[4]#dir#stp#nxt#data[0]#data[1]#data[2]#data[3]#clk#data[5]#data[6]#data[7]#clk#cmd#data[0]#data[1]#data[2]#data[3]#cd#gpio[47]#tx#rx#wp#gpio[51]#mdc#mdio</spirit:configurableElementValue>
        </spirit:configurableElementValues>
      </spirit:componentInstance>
      <spirit:componentInstance>
        <spirit:instanceName>xlslice_0</spirit:instanceName>
        <spirit:componentRef spirit:library="ip" spirit:name="xlslice" spirit:vendor="xilinx.com" spirit:version="1.0"/>
        <spirit:configurableElementValues>
          <spirit:configurableElementValue spirit:referenceId="bd:xciName">tutorial_xlslice_0_0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DOUT_WIDTH">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_TO">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_FROM">0</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_WIDTH">6</spirit:configurableElementValue>
        </spirit:configurableElementValues>
      </spirit:componentInstance>
      <spirit:componentInstance>
        <spirit:instanceName>xlslice_1</spirit:instanceName>
        <spirit:componentRef spirit:library="ip" spirit:name="xlslice" spirit:vendor="xilinx.com" spirit:version="1.0"/>
        <spirit:configurableElementValues>
          <spirit:configurableElementValue spirit:referenceId="bd:xciName">tutorial_xlslice_0_1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DOUT_WIDTH">4</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_TO">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_FROM">4</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_WIDTH">6</spirit:configurableElementValue>
        </spirit:configurableElementValues>
      </spirit:componentInstance>
      <spirit:componentInstance>
        <spirit:instanceName>xlslice_2</spirit:instanceName>
        <spirit:componentRef spirit:library="ip" spirit:name="xlslice" spirit:vendor="xilinx.com" spirit:version="1.0"/>
        <spirit:configurableElementValues>
          <spirit:configurableElementValue spirit:referenceId="bd:xciName">tutorial_xlslice_0_2</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DOUT_WIDTH">1</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_TO">5</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_FROM">5</spirit:configurableElementValue>
          <spirit:configurableElementValue spirit:referenceId="DIN_WIDTH">6</spirit:configurableElementValue>
        </spirit:configurableElementValues>
      </spirit:componentInstance>
    </spirit:componentInstances>
    <spirit:interconnections/>
    <spirit:adHocConnections>
      <spirit:adHocConnection>
        <spirit:name>SDIO1_CDN_1</spirit:name>
        <spirit:externalPortReference spirit:portRef="SDIO1_CDN"/>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="SDIO1_CDN"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>processing_system7_0_UART0_RTSN</spirit:name>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="UART0_RTSN"/>
        <spirit:externalPortReference spirit:portRef="UART0_RTSN"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>processing_system7_0_UART0_TX</spirit:name>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="UART0_TX"/>
        <spirit:externalPortReference spirit:portRef="UART0_TX"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>UART0_CTSN_1</spirit:name>
        <spirit:externalPortReference spirit:portRef="UART0_CTSN"/>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="UART0_CTSN"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>UART0_RX_1</spirit:name>
        <spirit:externalPortReference spirit:portRef="UART0_RX"/>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="UART0_RX"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>xlslice_0_Dout</spirit:name>
        <spirit:internalPortReference spirit:componentRef="xlslice_0" spirit:portRef="Dout"/>
        <spirit:externalPortReference spirit:portRef="BT_EN_SOC"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>xlslice_1_Dout</spirit:name>
        <spirit:internalPortReference spirit:componentRef="xlslice_1" spirit:portRef="Dout"/>
        <spirit:externalPortReference spirit:portRef="ARD_RELAY"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>processing_system7_0_SPI1_MOSI_O</spirit:name>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="SPI1_MOSI_O"/>
        <spirit:externalPortReference spirit:portRef="ARD_SPI1_MOSI"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>SPI1_MISO_I_1</spirit:name>
        <spirit:externalPortReference spirit:portRef="ARD_SPI1_MISO"/>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="SPI1_MISO_I"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>processing_system7_0_SPI1_SCLK_O</spirit:name>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="SPI1_SCLK_O"/>
        <spirit:externalPortReference spirit:portRef="ARD_SPI1_SCLK"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>processing_system7_0_SPI1_SS_O</spirit:name>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="SPI1_SS_O"/>
        <spirit:externalPortReference spirit:portRef="ARD_SPI1_SS"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>xlslice_2_Dout</spirit:name>
        <spirit:internalPortReference spirit:componentRef="xlslice_2" spirit:portRef="Dout"/>
        <spirit:externalPortReference spirit:portRef="ARD_SPI1_DC"/>
      </spirit:adHocConnection>
      <spirit:adHocConnection>
        <spirit:name>processing_system7_0_GPIO_O</spirit:name>
        <spirit:internalPortReference spirit:componentRef="processing_system7_0" spirit:portRef="GPIO_O"/>
        <spirit:internalPortReference spirit:componentRef="xlslice_0" spirit:portRef="Din"/>
        <spirit:internalPortReference spirit:componentRef="xlslice_1" spirit:portRef="Din"/>
        <spirit:internalPortReference spirit:componentRef="xlslice_2" spirit:portRef="Din"/>
      </spirit:adHocConnection>
    </spirit:adHocConnections>
    <spirit:hierConnections>
      <spirit:hierConnection spirit:interfaceRef="DDR/processing_system7_0_ddr">
        <spirit:activeInterface spirit:busRef="DDR" spirit:componentRef="processing_system7_0"/>
      </spirit:hierConnection>
      <spirit:hierConnection spirit:interfaceRef="FIXED_IO/processing_system7_0_fixed_io">
        <spirit:activeInterface spirit:busRef="FIXED_IO" spirit:componentRef="processing_system7_0"/>
      </spirit:hierConnection>
      <spirit:hierConnection spirit:interfaceRef="ARD_I2C1/processing_system7_0_IIC_1">
        <spirit:activeInterface spirit:busRef="IIC_1" spirit:componentRef="processing_system7_0"/>
      </spirit:hierConnection>
    </spirit:hierConnections>
  </spirit:design>

  <spirit:component xmlns:spirit="http://www.spiritconsortium.org/XMLSchema/SPIRIT/1685-2009">
    <spirit:vendor>xilinx.com</spirit:vendor>
    <spirit:library>Addressing/processing_system7_0</spirit:library>
    <spirit:name>processing_system7</spirit:name>
    <spirit:version>5.5</spirit:version>
    <spirit:addressSpaces>
      <spirit:addressSpace>
        <spirit:name>Data</spirit:name>
        <spirit:range>4G</spirit:range>
        <spirit:width>32</spirit:width>
        <spirit:segments/>
      </spirit:addressSpace>
    </spirit:addressSpaces>
  </spirit:component>

</bd:repository>
