<?xml version="1.0" encoding="UTF-8"?>
<spirit:design xmlns:xilinx="http://www.xilinx.com" xmlns:spirit="http://www.spiritconsortium.org/XMLSchema/SPIRIT/1685-2009" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
  <spirit:vendor>xilinx.com</spirit:vendor>
  <spirit:library>xci</spirit:library>
  <spirit:name>unknown</spirit:name>
  <spirit:version>1.0</spirit:version>
  <spirit:componentInstances>
    <spirit:componentInstance>
      <spirit:instanceName>System_processing_system7_0_0</spirit:instanceName>
      <spirit:componentRef spirit:vendor="xilinx.com" spirit:library="ip" spirit:name="processing_system7" spirit:version="5.4"/>
      <spirit:configurableElementValues>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_RAM_BASEADDR">0x00100000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_RAM_HIGHADDR">0x3FFFFFFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART0_BASEADDR">0xE0000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART0_HIGHADDR">0xE0000FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART1_BASEADDR">0xE0001000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART1_HIGHADDR">0xE0001FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C0_BASEADDR">0xE0004000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C0_HIGHADDR">0xE0004FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C1_BASEADDR">0xE0005000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C1_HIGHADDR">0xE0005FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_BASEADDR">0xE0006000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_HIGHADDR">0xE0006FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_BASEADDR">0xE0007000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_HIGHADDR">0xE0007FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN0_BASEADDR">0xE0008000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN0_HIGHADDR">0xE0008FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN1_BASEADDR">0xE0009000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN1_HIGHADDR">0xE0009FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_GPIO_BASEADDR">0xE000A000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_GPIO_HIGHADDR">0xE000AFFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_BASEADDR">0xE000B000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_HIGHADDR">0xE000BFFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_BASEADDR">0xE000C000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_HIGHADDR">0xE000CFFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SDIO0_BASEADDR">0xE0100000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SDIO0_HIGHADDR">0xE0100FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SDIO1_BASEADDR">0xE0101000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SDIO1_HIGHADDR">0xE0101FFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB0_BASEADDR">0xE0102000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB0_HIGHADDR">0xE0102fff</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB1_BASEADDR">0xE0103000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB1_HIGHADDR">0xE0103fff</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_BASEADDR">0xE0104000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_HIGHADDR">0xE0104fff</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_BASEADDR">0xE0105000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_HIGHADDR">0xE0105fff</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK_CLK0_BUF">true</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK_CLK1_BUF">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK_CLK2_BUF">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK_CLK3_BUF">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_FREQ_MHZ">533.333333</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_BANK_ADDR_COUNT">3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_ROW_ADDR_COUNT">15</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_COL_ADDR_COUNT">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CL">7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CWL">6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_T_RCD">7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_T_RP">7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_T_RC">48.75</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_T_RAS_MIN">35.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_T_FAW">40.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_AL">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_0">-0.073</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_1">-0.072</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_2">0.024</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_TO_CLK_DELAY_3">0.023</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_BOARD_DELAY0">0.294</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_BOARD_DELAY1">0.298</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_BOARD_DELAY2">0.338</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_BOARD_DELAY3">0.334</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_0_LENGTH_MM">50.05</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_1_LENGTH_MM">50.43</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_2_LENGTH_MM">50.10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_3_LENGTH_MM">50.01</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_0_LENGTH_MM">49.59</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_1_LENGTH_MM">51.74</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_2_LENGTH_MM">50.32</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_3_LENGTH_MM">48.55</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_0_LENGTH_MM">39.7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_1_LENGTH_MM">39.7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_2_LENGTH_MM">54.14</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_3_LENGTH_MM">54.14</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_0_PACKAGE_LENGTH">101.239</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_1_PACKAGE_LENGTH">79.5025</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_2_PACKAGE_LENGTH">60.536</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_3_PACKAGE_LENGTH">71.7715</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_0_PACKAGE_LENGTH">104.5365</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_1_PACKAGE_LENGTH">70.676</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_2_PACKAGE_LENGTH">59.1615</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_3_PACKAGE_LENGTH">81.319</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_0_PACKAGE_LENGTH">54.563</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_1_PACKAGE_LENGTH">54.563</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_2_PACKAGE_LENGTH">54.563</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_3_PACKAGE_LENGTH">54.563</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_0_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_1_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_2_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQS_3_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_0_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_1_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_2_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DQ_3_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_0_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_1_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_2_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_3_PROPOGATION_DELAY">160</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_0">-0.073</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_1">-0.072</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_2">0.024</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_DDR_DQS_TO_CLK_DELAY_3">0.023</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_DDR_BOARD_DELAY0">0.294</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_DDR_BOARD_DELAY1">0.298</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_DDR_BOARD_DELAY2">0.338</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_DDR_BOARD_DELAY3">0.334</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CPU_CPU_6X4X_MAX_RANGE">667</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CRYSTAL_PERIPHERAL_FREQMHZ">33.333333</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_APU_PERIPHERAL_FREQMHZ">666.666666</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DCI_PERIPHERAL_FREQMHZ">10.159</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_PERIPHERAL_FREQMHZ">200.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_PERIPHERAL_FREQMHZ">100</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB0_PERIPHERAL_FREQMHZ">60</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB1_PERIPHERAL_FREQMHZ">60</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SDIO_PERIPHERAL_FREQMHZ">50</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART_PERIPHERAL_FREQMHZ">50</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI_PERIPHERAL_FREQMHZ">166.666666</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN_PERIPHERAL_FREQMHZ">100</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN0_PERIPHERAL_FREQMHZ">-1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN1_PERIPHERAL_FREQMHZ">-1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C_PERIPHERAL_FREQMHZ">25</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_WDT_PERIPHERAL_FREQMHZ">133.333333</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC_PERIPHERAL_FREQMHZ">50</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK0_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK1_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK2_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK0_PERIPHERAL_FREQMHZ">133.333333</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK1_PERIPHERAL_FREQMHZ">133.333333</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK2_PERIPHERAL_FREQMHZ">133.333333</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PCAP_PERIPHERAL_FREQMHZ">200</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TPIU_PERIPHERAL_FREQMHZ">200</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FPGA0_PERIPHERAL_FREQMHZ">100</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FPGA1_PERIPHERAL_FREQMHZ">100</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FPGA2_PERIPHERAL_FREQMHZ">33.333333</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FPGA3_PERIPHERAL_FREQMHZ">50</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_APU_PERIPHERAL_FREQMHZ">666.666687</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_ACT_DDR_FREQ_MHZ">533.333374</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_DCI_PERIPHERAL_FREQMHZ">10.158731</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_QSPI_PERIPHERAL_FREQMHZ">200.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_SMC_PERIPHERAL_FREQMHZ">10.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_ENET0_PERIPHERAL_FREQMHZ">125.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_ENET1_PERIPHERAL_FREQMHZ">10.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_USB0_PERIPHERAL_FREQMHZ">60</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_USB1_PERIPHERAL_FREQMHZ">60</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_SDIO_PERIPHERAL_FREQMHZ">50.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_UART_PERIPHERAL_FREQMHZ">50.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_SPI_PERIPHERAL_FREQMHZ">10.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_CAN_PERIPHERAL_FREQMHZ">10.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_I2C_PERIPHERAL_FREQMHZ">50</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_WDT_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_TTC_PERIPHERAL_FREQMHZ">50</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_PCAP_PERIPHERAL_FREQMHZ">200.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_TPIU_PERIPHERAL_FREQMHZ">200.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_FPGA0_PERIPHERAL_FREQMHZ">100.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_FPGA1_PERIPHERAL_FREQMHZ">100.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_FPGA2_PERIPHERAL_FREQMHZ">33.333336</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_FPGA3_PERIPHERAL_FREQMHZ">50.000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_TTC0_CLK0_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_TTC0_CLK1_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_TTC0_CLK2_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_TTC1_CLK0_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_TTC1_CLK1_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ACT_TTC1_CLK2_PERIPHERAL_FREQMHZ">111.111115</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CLK0_FREQ">100000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CLK1_FREQ">100000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CLK2_FREQ">33333336</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CLK3_FREQ">50000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_OVERRIDE_BASIC_CLOCK">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CPU_PERIPHERAL_DIVISOR0">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PERIPHERAL_DIVISOR0">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_PERIPHERAL_DIVISOR0">5</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SDIO_PERIPHERAL_DIVISOR0">20</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART_PERIPHERAL_DIVISOR0">20</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN_PERIPHERAL_DIVISOR1">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK0_PERIPHERAL_DIVISOR0">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK1_PERIPHERAL_DIVISOR0">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK2_PERIPHERAL_DIVISOR0">30</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK3_PERIPHERAL_DIVISOR0">20</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK0_PERIPHERAL_DIVISOR1">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK1_PERIPHERAL_DIVISOR1">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK2_PERIPHERAL_DIVISOR1">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK3_PERIPHERAL_DIVISOR1">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_PERIPHERAL_DIVISOR0">8</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_PERIPHERAL_DIVISOR1">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_PERIPHERAL_DIVISOR1">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TPIU_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DCI_PERIPHERAL_DIVISOR0">35</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DCI_PERIPHERAL_DIVISOR1">3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PCAP_PERIPHERAL_DIVISOR0">5</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK0_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK1_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK2_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK0_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK1_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK2_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_WDT_PERIPHERAL_DIVISOR0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ARMPLL_CTRL_FBDIV">40</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_IOPLL_CTRL_FBDIV">30</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDRPLL_CTRL_FBDIV">32</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CPU_CPU_PLL_FREQMHZ">1333.333</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_IO_IO_PLL_FREQMHZ">1000.000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_DDR_PLL_FREQMHZ">1066.667</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_PERIPHERAL_VALID">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SDIO_PERIPHERAL_VALID">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI_PERIPHERAL_VALID">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN_PERIPHERAL_VALID">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_CAN0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_CAN1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_ENET0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_ENET1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_GPIO">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_I2C0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_I2C1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_PJTAG">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_SDIO0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_CD_SDIO0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_WP_SDIO0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_SDIO1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_CD_SDIO1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_WP_SDIO1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_SPI0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_SPI1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_UART0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_UART1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_MODEM_UART0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_MODEM_UART1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_TTC0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_TTC1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_WDT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_TRACE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_M_AXI_GP0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_M_AXI_GP1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_S_AXI_GP0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_S_AXI_GP1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_S_AXI_ACP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_S_AXI_HP0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_S_AXI_HP1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_S_AXI_HP2">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_S_AXI_HP3">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP0_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP1_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_GP0_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_GP1_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_ACP_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP0_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP1_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP2_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP3_FREQMHZ">10</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_DMA0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_DMA1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_DMA2">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_DMA3">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_TRACE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_PIPELINE_WIDTH">8</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_INCLUDE_TRACE_BUFFER">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_BUFFER_FIFO_SIZE">128</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_TRACE_DATA_EDGE_DETECTOR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_BUFFER_CLOCK_DELAY">12</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_CROSS_TRIGGER">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FTM_CTI_IN0">DISABLED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FTM_CTI_IN1">DISABLED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FTM_CTI_IN2">DISABLED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FTM_CTI_IN3">DISABLED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FTM_CTI_OUT0">DISABLED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FTM_CTI_OUT1">DISABLED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FTM_CTI_OUT2">DISABLED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FTM_CTI_OUT3">DISABLED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_DEBUG">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_CR_FABRIC">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_AXI_FABRIC_IDLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_DDR_BYPASS">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_FABRIC_INTERRUPT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_PROC_EVENT_BUS">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_EXPANDED_IOP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_HIGH_OCM">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_PS_SLCR_REGISTERS">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_EXPANDED_PS_SLCR_REGISTERS">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_CORESIGHT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_EMIO_SRAM_INT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_GPIO_EMIO_GPIO_WIDTH">64</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART0_BAUD_RATE">115200</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART1_BAUD_RATE">115200</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_4K_TIMER">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP0_ID_WIDTH">12</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP0_ENABLE_STATIC_REMAP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP0_SUPPORT_NARROW_BURST">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP0_THREAD_ID_WIDTH">12</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP1_ID_WIDTH">12</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP1_ENABLE_STATIC_REMAP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP1_SUPPORT_NARROW_BURST">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_M_AXI_GP1_THREAD_ID_WIDTH">12</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_GP0_ID_WIDTH">6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_GP1_ID_WIDTH">6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_ACP_ID_WIDTH">3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_INCLUDE_ACP_TRANS_CHECK">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USE_DEFAULT_ACP_USER_VAL">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_ACP_ARUSER_VAL">31</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_ACP_AWUSER_VAL">31</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP0_ID_WIDTH">6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP0_DATA_WIDTH">64</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP1_ID_WIDTH">6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP1_DATA_WIDTH">64</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP2_ID_WIDTH">6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP2_DATA_WIDTH">64</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP3_ID_WIDTH">6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_S_AXI_HP3_DATA_WIDTH">64</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NUM_F2P_INTR_INPUTS">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_DDR">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_SMC">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_QSPI">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CAN0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CAN1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_ENET0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_ENET1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_GPIO">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_I2C0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_I2C1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_PJTAG">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_SDIO0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_SDIO1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_SPI0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_SPI1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_UART0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_UART1">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_MODEM_UART0">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_MODEM_UART1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_TTC0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_TTC1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_WDT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_TRACE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_USB0">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_USB1">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DQ_WIDTH">32</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DQS_WIDTH">4</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DM_WIDTH">4</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_PRIMITIVE">54</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CLK0_PORT">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CLK1_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CLK2_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CLK3_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_RST0_PORT">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_RST1_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_RST2_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_RST3_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CLKTRIG0_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CLKTRIG1_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CLKTRIG2_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_EN_CLKTRIG3_PORT">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC_ABORT_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC0_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC1_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC2_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC3_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC4_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC5_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC6_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_DMAC7_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_SMC_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_QSPI_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_CTI_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_GPIO_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_USB0_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_ENET0_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_SDIO0_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_I2C0_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_SPI0_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_UART0_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_CAN0_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_USB1_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_ENET1_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_SDIO1_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_I2C1_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_SPI1_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_UART1_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_P2F_CAN1_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_IRQ_F2P_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_IRQ_F2P_MODE">DIRECT</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CORE0_FIQ_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CORE0_IRQ_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CORE1_FIQ_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CORE1_IRQ_INTR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_VALUE_SILVERSION">3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_IMPORT_BOARD_PRESET">None</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PERIPHERAL_BOARD_PRESET">part0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PRESET_BANK0_VOLTAGE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PRESET_BANK1_VOLTAGE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_ADV_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_MEMORY_TYPE">DDR 3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_ECC">Disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_BUS_WIDTH">32 Bit</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_BL">8</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_HIGH_TEMP">Normal (0-85)</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_PARTNO">MT41K256M16 RE-125</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DRAM_WIDTH">16 Bits</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_DEVICE_CAPACITY">4096 MBits</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_SPEED_BIN">DDR3_1066F</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_TRAIN_WRITE_LEVEL">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_TRAIN_READ_GATE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_TRAIN_DATA_EYE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_CLOCK_STOP_EN">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_DDR_USE_INTERNAL_VREF">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PRIORITY_WRITEPORT_0">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PRIORITY_WRITEPORT_1">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PRIORITY_WRITEPORT_2">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PRIORITY_WRITEPORT_3">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PRIORITY_READPORT_0">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PRIORITY_READPORT_1">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PRIORITY_READPORT_2">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PRIORITY_READPORT_3">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PORT0_HPR_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PORT1_HPR_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PORT2_HPR_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PORT3_HPR_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_HPRLPR_QUEUE_PARTITION">HPR(0)/LPR(32)</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_LPR_TO_CRITICAL_PRIORITY_LEVEL">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_HPR_TO_CRITICAL_PRIORITY_LEVEL">15</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_WRITE_TO_CRITICAL_PRIORITY_LEVEL">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_NAND_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_GRP_D8_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_GRP_D8_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_NOR_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_A25_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_A25_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_CS0_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_CS0_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_SRAM_CS0_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_SRAM_CS0_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_CS1_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_CS1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_SRAM_CS1_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_SRAM_CS1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_SRAM_INT_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_GRP_SRAM_INT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_QSPI_IO">MIO 1 .. 6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_GRP_SINGLE_SS_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_GRP_SINGLE_SS_IO">MIO 1 .. 6</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_GRP_SS1_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_GRP_SS1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_GRP_IO1_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_GRP_IO1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_GRP_FBCLK_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_GRP_FBCLK_IO">MIO 8</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_INTERNAL_HIGHADDRESS">0xFCFFFFFF</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_ENET0_IO">MIO 16 .. 27</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_GRP_MDIO_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_GRP_MDIO_IO">MIO 52 .. 53</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_RESET_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_RESET_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_ENET1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_GRP_MDIO_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_GRP_MDIO_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_RESET_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_RESET_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD0_SD0_IO">MIO 40 .. 45</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD0_GRP_CD_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD0_GRP_CD_IO">MIO 46</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD0_GRP_WP_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD0_GRP_WP_IO">MIO 50</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD0_GRP_POW_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD0_GRP_POW_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD1_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD1_SD1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD1_GRP_CD_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD1_GRP_CD_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD1_GRP_WP_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD1_GRP_WP_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD1_GRP_POW_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SD1_GRP_POW_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART0_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART0_UART0_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART0_GRP_FULL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART0_GRP_FULL_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART1_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART1_UART1_IO">MIO 48 .. 49</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART1_GRP_FULL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART1_GRP_FULL_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_SPI0_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_GRP_SS0_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_GRP_SS0_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_GRP_SS1_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_GRP_SS1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_GRP_SS2_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI0_GRP_SS2_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_SPI1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_GRP_SS0_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_GRP_SS0_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_GRP_SS1_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_GRP_SS1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_GRP_SS2_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI1_GRP_SS2_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN0_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN0_CAN0_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN0_GRP_CLK_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN0_GRP_CLK_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN1_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN1_CAN1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN1_GRP_CLK_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN1_GRP_CLK_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_TRACE_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_2BIT_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_2BIT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_4BIT_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_4BIT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_8BIT_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_8BIT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_16BIT_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_16BIT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_32BIT_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TRACE_GRP_32BIT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_WDT_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_WDT_WDT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_TTC0_IO">EMIO</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_TTC1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PJTAG_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PJTAG_PJTAG_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB0_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB0_USB0_IO">MIO 28 .. 39</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB0_RESET_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB0_RESET_IO">MIO 7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB1_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB1_USB1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB1_RESET_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB1_RESET_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C0_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C0_I2C0_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C0_GRP_INT_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C0_GRP_INT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C0_RESET_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C0_RESET_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C1_PERIPHERAL_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C1_I2C1_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C1_GRP_INT_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C1_GRP_INT_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C1_RESET_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C1_RESET_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_GPIO_PERIPHERAL_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_GPIO_MIO_GPIO_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_GPIO_MIO_GPIO_IO">MIO</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_GPIO_EMIO_GPIO_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_GPIO_EMIO_GPIO_IO">&lt;Select></spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_APU_CLK_RATIO_ENABLE">6:2:1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_PERIPHERAL_FREQMHZ">1000 Mbps</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_PERIPHERAL_FREQMHZ">1000 Mbps</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CPU_PERIPHERAL_CLKSRC">ARM PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DDR_PERIPHERAL_CLKSRC">DDR PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_QSPI_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SDIO_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UART_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SPI_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK0_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK1_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK2_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FCLK3_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET0_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET1_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN0_PERIPHERAL_CLKSRC">External</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_CAN1_PERIPHERAL_CLKSRC">External</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TPIU_PERIPHERAL_CLKSRC">External</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK0_PERIPHERAL_CLKSRC">CPU_1X</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK1_PERIPHERAL_CLKSRC">CPU_1X</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC0_CLK2_PERIPHERAL_CLKSRC">CPU_1X</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK0_PERIPHERAL_CLKSRC">CPU_1X</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK1_PERIPHERAL_CLKSRC">CPU_1X</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_TTC1_CLK2_PERIPHERAL_CLKSRC">CPU_1X</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_WDT_PERIPHERAL_CLKSRC">CPU_1X</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_DCI_PERIPHERAL_CLKSRC">DDR PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PCAP_PERIPHERAL_CLKSRC">IO PLL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_USB_RESET_POLARITY">Active Low</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_ENET_RESET_POLARITY">Active Low</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_I2C_RESET_POLARITY">Active Low</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_0_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_0_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_0_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_0_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_1_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_1_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_1_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_1_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_2_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_2_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_2_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_2_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_3_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_3_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_3_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_3_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_4_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_4_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_4_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_4_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_5_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_5_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_5_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_5_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_6_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_6_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_6_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_6_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_7_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_7_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_7_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_7_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_8_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_8_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_8_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_8_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_9_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_9_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_9_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_9_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_10_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_10_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_10_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_10_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_11_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_11_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_11_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_11_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_12_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_12_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_12_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_12_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_13_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_13_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_13_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_13_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_14_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_14_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_14_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_14_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_15_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_15_IOTYPE">LVCMOS 3.3V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_15_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_15_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_16_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_16_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_16_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_16_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_17_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_17_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_17_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_17_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_18_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_18_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_18_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_18_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_19_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_19_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_19_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_19_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_20_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_20_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_20_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_20_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_21_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_21_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_21_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_21_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_22_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_22_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_22_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_22_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_23_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_23_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_23_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_23_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_24_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_24_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_24_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_24_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_25_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_25_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_25_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_25_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_26_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_26_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_26_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_26_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_27_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_27_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_27_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_27_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_28_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_28_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_28_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_28_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_29_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_29_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_29_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_29_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_30_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_30_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_30_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_30_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_31_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_31_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_31_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_31_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_32_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_32_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_32_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_32_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_33_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_33_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_33_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_33_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_34_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_34_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_34_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_34_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_35_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_35_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_35_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_35_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_36_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_36_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_36_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_36_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_37_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_37_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_37_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_37_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_38_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_38_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_38_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_38_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_39_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_39_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_39_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_39_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_40_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_40_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_40_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_40_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_41_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_41_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_41_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_41_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_42_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_42_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_42_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_42_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_43_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_43_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_43_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_43_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_44_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_44_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_44_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_44_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_45_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_45_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_45_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_45_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_46_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_46_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_46_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_46_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_47_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_47_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_47_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_47_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_48_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_48_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_48_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_48_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_49_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_49_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_49_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_49_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_50_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_50_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_50_DIRECTION">in</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_50_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_51_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_51_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_51_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_51_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_52_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_52_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_52_DIRECTION">out</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_52_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_53_PULLUP">disabled</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_53_IOTYPE">LVCMOS 1.8V</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_53_DIRECTION">inout</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_53_SLEW">slow</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.preset">Default*</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_UIPARAM_GENERATE_SUMMARY">NA</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_TREE_PERIPHERALS">GPIO#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#Quad SPI Flash#USB Reset#Quad SPI Flash#GPIO#GPIO#GPIO#GPIO#GPIO#GPIO#GPIO#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#Enet 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#USB 0#SD 0#SD 0#SD 0#SD 0#SD 0#SD 0#SD 0#GPIO#UART 1#UART 1#SD 0#GPIO#Enet 0#Enet 0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_MIO_TREE_SIGNALS">gpio[0]#qspi0_ss_b#qspi0_io[0]#qspi0_io[1]#qspi0_io[2]#qspi0_io[3]#qspi0_sclk#reset#qspi_fbclk#gpio[9]#gpio[10]#gpio[11]#gpio[12]#gpio[13]#gpio[14]#gpio[15]#tx_clk#txd[0]#txd[1]#txd[2]#txd[3]#tx_ctl#rx_clk#rxd[0]#rxd[1]#rxd[2]#rxd[3]#rx_ctl#data[4]#dir#stp#nxt#data[0]#data[1]#data[2]#data[3]#clk#data[5]#data[6]#data[7]#clk#cmd#data[0]#data[1]#data[2]#data[3]#cd#gpio[47]#tx#rx#wp#gpio[51]#mdc#mdio</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PS7_SI_REV">PRODUCTION</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FPGA_FCLK0_ENABLE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FPGA_FCLK1_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FPGA_FCLK2_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_FPGA_FCLK3_ENABLE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS0_T_TR">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS0_T_PC">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS0_T_WP">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS0_T_CEOE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS0_T_WC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS0_T_RC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS0_WE_TIME">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS1_T_TR">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS1_T_PC">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS1_T_WP">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS1_T_CEOE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS1_T_WC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS1_T_RC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_SRAM_CS1_WE_TIME">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS0_T_TR">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS0_T_PC">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS0_T_WP">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS0_T_CEOE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS0_T_WC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS0_T_RC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS0_WE_TIME">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS1_T_TR">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS1_T_PC">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS1_T_WP">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS1_T_CEOE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS1_T_WC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS1_T_RC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NOR_CS1_WE_TIME">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_CYCLES_T_RR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_CYCLES_T_AR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_CYCLES_T_CLR">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_CYCLES_T_WP">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_CYCLES_T_REA">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_CYCLES_T_WC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_NAND_CYCLES_T_RC">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_CYCLE_T0">NA</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_CYCLE_T1">NA</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_CYCLE_T2">NA</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_CYCLE_T3">NA</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_CYCLE_T4">NA</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_CYCLE_T5">NA</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_SMC_CYCLE_T6">NA</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.PCW_PACKAGE_NAME">clg400</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Component_Name">System_processing_system7_0_0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.ARCHITECTURE">zynq</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.DEVICE">xc7z010</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.PACKAGE">clg400</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.SPEEDGRADE">-1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.PREFHDL">VERILOG</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.SIMULATOR_LANGUAGE">MIXED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.USE_RDI_CUSTOMIZATION">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.USE_RDI_GENERATION">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.USER_REPO_PATHS"/>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.BOARD">em.avnet.com:microzed_7010:part0:1.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.MANAGED">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SWVERSION">2014.2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.IPREVISION">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SYNTHESISFLOW">OUT_OF_CONTEXT</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.OUTPUTDIR">.</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SHAREDDIR">../../../../ipshared</spirit:configurableElementValue>
      </spirit:configurableElementValues>
    </spirit:componentInstance>
  </spirit:componentInstances>
</spirit:design>
