- Main Page
- Data Structures
- Files
- Directories

- Data Structures
- Data Fields

# XIsf_WriteParam Struct Reference

`#include <xilisf.h>`

## Data Fields
u32 | Address
u8 * | WritePtr
u32 | NumBytes

## Detailed Description

The following structure definition specifies the operational parameters to be passed to the XIsf_Write API while performing Normal write (XISF_WRITE) and OTP write (XISF_OTP_WRITE) operations.

## Field Documentation

u32 XIsf_WriteParam::Address

| Address in the Serial Flash

u32 XIsf_WriteParam::NumBytes

| Number of bytes to be written to the Serial Flash

u8* XIsf_WriteParam::WritePtr

| Pointer to the data to be written to the Serial Flash

The documentation for this struct was generated from the following file:

- xilisf.h