- Main Page
- Data Structures
- Files
- Directories

- Data Structures
- Data Fields

# XIsf_BufferReadParam Struct Reference

`#include <xilisf.h>`

## Data Fields
u8 | BufferNum
u8 * | ReadPtr
u32 | ByteOffset
u32 | NumBytes

## Detailed Description

The following structure definition specifies the operational parameters to be passed to the XIsf_Read API while reading data from the Internal SRAM buffer of Flash using XISF_BUFFER_READ or XISF_FAST_BUFFER_READ commands in Atmel Serial Flash.

## Field Documentation

u8 XIsf_BufferReadParam::BufferNum

| SRAM buffer number of Serial Flash

u32 XIsf_BufferReadParam::ByteOffset

| Byte offset in the SRAM buffer from where the first byte is read

u32 XIsf_BufferReadParam::NumBytes

| Number of bytes to be read from the buffer

u8* XIsf_BufferReadParam::ReadPtr

| Read buffer pointer where data read from the SRAM buffer is stored

The documentation for this struct was generated from the following file:

- xilisf.h