- Main Page
- Data Structures
- Files
- Directories

- Data Structures
- Data Fields

# XIsf_BufferWriteParam Struct Reference

`#include <xilisf.h>`

## Data Fields
u8 | BufferNum
u8 * | WritePtr
u32 | ByteOffset
u32 | NumBytes

## Detailed Description

The following structure definition specifies the operational parameters to be passed to the XIsf_Write API while writing data to the internal SRAM buffer of the Atmel Serial Flash (XISF_BUFFER_WRITE).

## Field Documentation

u8 XIsf_BufferWriteParam::BufferNum

| SRAM buffer number of Serial Flash

u32 XIsf_BufferWriteParam::ByteOffset

| Byte offset in the buffer from which the data is written

u32 XIsf_BufferWriteParam::NumBytes

| Number of bytes to be written into the buffer

u8* XIsf_BufferWriteParam::WritePtr

| Pointer to the data to be written into the Serial Flash SRAM Buffer

The documentation for this struct was generated from the following file:

- xilisf.h